
Programing:

Refer to page 915 for programing.

1K pull-up resistor at SWCLK pin.

ATSAMD11 uses serial wire debugger (SWD) interface for programing and debugging.

Use cortex Debug Connector (10-pin). The diagram is as follows



(ref: Datasheet, page 917)